# Midterm

Tharson Sutharson

|  |  |
| --- | --- |
| R1 | R2 |
| service timestamps debug datetime msec  service timestamps log datetime msec  service password-encryption  platform qfp utilization monitor load 80  platform punt-keepalive disable-kernel-core  !  hostname R1  !  boot-start-marker  boot-end-marker  !  !  !  no aaa new-model  !  !  !  !  !  !  !  no ip domain lookup  ip domain name lab.com  !  !  !  login on-success log  !  !  !  !  !  !  !  subscriber templating  multilink bundle-name authenticated  !  !  !  !  !  !  license udi pid C8200L-1N-4T sn FJC27291G3Y  memory free low-watermark processor 67482  !  diagnostic bootup level minimal  !  spanning-tree extend system-id  !  username admin password 7 060506324F41  !  redundancy  mode none  !  !  !  !  !  !  !  !  interface Loopback0  ip address 209.166.74.1 255.255.255.0  !  interface GigabitEthernet0/0/0  ip address 10.74.254.2 255.255.255.252  ip access-group R1-SEC in  ip ospf hello-interval 30  ip ospf priority 50  negotiation auto  !  interface GigabitEthernet0/0/1  ip address 192.168.74.1 255.255.255.0  negotiation auto  !  interface GigabitEthernet0/0/2  no ip address  negotiation auto  !  interface GigabitEthernet0/0/3  no ip address  negotiation auto  !  interface Serial0/1/0  no ip address  !  interface Serial0/1/1  no ip address  !  router ospf 74  router-id 1.0.0.1  auto-cost reference-bandwidth 1000  network 192.168.74.0 0.0.0.255 area 0  !  no ip http server  ip http secure-server  ip forward-protocol nd  !  !  ip access-list extended R1-SEC  10 permit tcp any host 209.166.74.1 eq 22  !  !  !  !  control-plane  !  !  line con 0  stopbits 1  line aux 0  line vty 0 4  login local  transport input ssh  line vty 5 14  login  transport input ssh  !  !  !  !  !  !  !  end | service timestamps debug datetime msec  service timestamps log datetime msec  service password-encryption  !  hostname R2  !  boot-start-marker  boot-end-marker  !  !  ! card type command needed for slot/vwic-slot 0/1  !  no aaa new-model  memory-size iomem 15  !  !  !  --More--  \*Jan 23 15:56:01.263: %SYS-5-CONFIG\_I: Configured from console ! e  !  !  !  !  !  !  !  !  !  !  no ip domain lookup  ip domain name lab.com  ip cef  no ipv6 cef  !  multilink bundle-name authenticated  !  !  !  !  !  !  cts logging verbose  !  !  voice-card 0  !  !  !  !  !  !  !  !  license udi pid CISCO2901/K9 sn FJC2121A174  license accept end user agreement  license boot module c2900 technology-package securityk9  hw-module pvdm 0/0  !  hw-module pvdm 0/1  !  !  !  username admin password 7 094F471A1A0A  !  redundancy  !  !  !  !  !  !  !  !  !  !  !  !  !  !  !  interface Loopback0  ip address 209.165.74.1 255.255.255.0  !  interface Embedded-Service-Engine0/0  no ip address  shutdown  !  interface GigabitEthernet0/0  ip address 10.74.254.1 255.255.255.252  ip access-group R2-SEC in  ip ospf hello-interval 30  ip ospf priority 55  duplex auto  speed auto  !  interface GigabitEthernet0/1  ip address 10.74.1.1 255.255.255.0  duplex auto  speed auto  !  interface Serial0/0/0  no ip address  shutdown  clock rate 2000000  !  interface Serial0/0/1  no ip address  shutdown  !  router ospf 74  router-id 2.0.0.2  auto-cost reference-bandwidth 1000  network 10.74.1.0 0.0.0.255 area 0  !  ip forward-protocol nd  !  no ip http server  no ip http secure-server  !  ip route 0.0.0.0 0.0.0.0 Loopback0  !  ip access-list extended R2-SEC  deny tcp any host 209.165.74.1 eq 22  permit ip any any  !  !  !  !  control-plane  !  !  voice-port 0/2/0  !  voice-port 0/2/1  !  voice-port 0/3/0  !  voice-port 0/3/1  !  !  !  !  !  mgcp behavior rsip-range tgcp-only  mgcp behavior comedia-role none  mgcp behavior comedia-check-media-src disable  mgcp behavior comedia-sdp-force disable  !  mgcp profile default  !  !  !  !  !  !  !  gatekeeper  shutdown  !  !  banner motd ^C Authorized Users Only! ^C  !  line con 0  line aux 0  line 2  no activation-character  no exec  transport preferred none  transport output pad telnet rlogin lapb-ta mop udptn v120 ssh  stopbits 1  line vty 0 4  login local  transport input ssh  !  scheduler allocate 20000 1000  !  end |

R1 Screenshot

A screenshot of a computer

Description automatically generated

A screenshot of a computer

Description automatically generated

# R2 Screenshot

A screenshot of a computer program

Description automatically generated

A screenshot of a computer screen

Description automatically generated

A screenshot of a computer program

Description automatically generated